**REFERENCES**

[1] G. Giannakakis, D. Manousos, F. Chiarugi, “Stress and anxiety detection using facial cues from videos,” Biomedical Signal processing and Control”, vol. 31, pp. 89-101, January 2017.

[2] T. Jick and R. Payne, “Stress at work,” Journal of Management Education, vol. 5, no. 3, pp. 50-56, 1980.

[3] Nisha Raichur, Nidhi Lonakadi, Priyanka Mural, “Detection of Stress Using Image Processing and Machine Learning Techniques”, vol.9, no. 3S, July 2017.

[4] Bhattacharyya, R., & Basu, S. (2018). Retrieved from ‘The Economic Times’.

[5] OSMI Mental Health in Tech Survey Dataset, 2017

[6] U. S. Reddy, A. V. Thota and A. Dharun, "Machine Learning Techniques for Stress Prediction in Working Employees," 2018 IEEE International Conference on Computational Intelligence and Computing Research (ICCIC), Madurai, India, 2018, pp. 1-4.

[7] https://www.kaggle.com/qiriro/stress

[8] Communications, N.. World health report. 2001. URL: http://www.who.int/whr/2001/media\_centre/press\_release/en/.

[9] Bakker, J., Holenderski, L., Kocielnik, R., Pechenizkiy, M., Sidorova, N.. Stess@ work: From measuring stress to its understanding, prediction and handling with personalized coaching. In: Proceedings of the 2nd ACM SIGHIT International health informatics symposium. ACM; 2012, p. 673–678.

[10] Deng, Y., Wu, Z., Chu, C.H., Zhang, Q., Hsu, D.F.. Sensor feature selection and combination for stress identification using combinatorial fusion. International Journal of Advanced Robotic Systems 2013;10(8):306.

[11] Ghaderi, A., Frounchi, J., Farnam, A.. Machine learning-based signal processing using physiological signals for stress detection. In: 2015 22nd Iranian Conference on Biomedical Engineering (ICBME). 2015, p. 93–98.

[12] Villarejo, M.V., Zapirain, B.G., Zorrilla, A.M.. A stress sensor based on galvanic skin response (gsr) controlled by zigbee. Sensors 2012; 12(5):6075–6101.

[13] Liu, D., Ulrich, M.. Listen to your heart: Stress prediction using consumer heart rate sensors 2015;.

[14] Nakashima, Y., Kim, J., Flutura, S., Seiderer, A., Andre, E.. Stress recognition in daily work. In: ´ International Symposium on Pervasive Computing Paradigms for Mental Health. Springer; 2015, p. 23–33.

[15] Xu, Q., Nwe, T.L., Guan, C.. Cluster-based analysis for personalized stress evaluation using physiological signals. IEEE journal of biomedical and health informatics 2015;19(1):275–281.

[16] Tanev, G., Saadi, D.B., Hoppe, K., Sorensen, H.B.. Classification of acute stress using linear and non-linear heart rate variability analysis derived from sternal ecg. In: Engineering in Medicine and Biology Society (EMBC), 2014 36th Annual International Conference of the IEEE. IEEE; 2014, p. 3386–3389.

[17] Gjoreski, M., Gjoreski, H., Lustrek, M., Gams, M.. Continuous stress detection using a wrist device: in laboratory and real life. In: Proceedings of the 2016 ACM International Joint Conference on Pervasive and Ubiquitous Computing: Adjunct. ACM; 2016, p. 1185–1193.

[18] Palanisamy, K., Murugappan, M., Yaacob, S.. Multiple physiological signal-based human stress identification using non-linear classifiers.Elektronika ir elektrotechnika 2013;19(7):80–85.

[19] Widanti, N., Sumanto, B., Rosa, P., Miftahudin, M.F.. Stress level detection using heart rate, blood pressure, and gsr and stress therapy by utilizing infrared. In: Industrial Instrumentation and Control (ICIC), 2015 International Conference on. IEEE; 2015, p. 275–279.

[20] Sioni, R., Chittaro, L.. Stress detection using physiological sensors. Computer 2015;48(10):26–33.

[21] Zenonos, A., Khan, A., Kalogridis, G., Vatsikas, S., Lewis, T., Sooriyabandara, M.. Healthyoffice: Mood recognition at work using smartphones and wearable sensors. In: Pervasive Computing and Communication Workshops (PerCom Workshops), 2016 IEEE International Conference on. IEEE; 2016, p. 1–6.

[22] Selvaraj, N.. Psychological acute stress measurement using a wireless adhesive biosensor. In: 2015 37th Annual International Conference of the IEEE Engineering in Medicine and Biology Society (EMBC). 2015, p. 3137–3140.

[23] Vadana, D.P., Kottayil, S.K.. Energy-aware intelligent controller for dynamic energy management on smart microgrid. In: Power and Energy Systems Conference: Towards Sustainable Energy, 2014. IEEE; 2014, p. 1–7.

[24] Rajagopalan, S.S., Murthy, O.R., Goecke, R., Rozga, A.. Play with memeasuring a child’s engagement in a social interaction. In: Automatic Face and Gesture Recognition (FG), 2015 11th IEEE International Conference and Workshops on; vol. 1. IEEE; 2015, p. 1–8.

[25] Koldijk, S., Neerincx, M.A., Kraaij, W.. Detecting work stress in offices by combining unobtrusive sensors. IEEE Transactions on Affective Computing 2016;.

[26] Koldijk, S., Sappelli, M., Verberne, S., Neerincx, M.A., Kraaij, W.. The swell knowledge work dataset for stress and user modeling research. In: Proceedings of the 16th International Conference on Multimodal Interaction; ICMI ’14. New York, NY, USA: ACM. ISBN 978-1-4503-2885-2; 2014, p. 291–298. URL: http://doi.acm.org/10.1145/2663204.2663257. doi:10.1145/2663204.2663257.

[27] Yoder, N.. Peakfinder. Internet: http://www mathworks com-/matlabcentral/fileexchange/25500 2011;.